1078	Emluator machining
1296	Clamp Current_position：
1300	Saw Curren_position：
1301	Backboard Curren_postion：
1302	Surplus mode
1373    FOFC
1197	Front Surplus 
1200	Back Surplus 
1307	CYC number：
1305	Emluator times
1306	Emluator operation
1051	Total groups
1082	Continuous
1054	Start 
1084	Current 
1036	System status: not started
1225	Alarm：None
1022	Alarm Reset
1287	Position display
1037	Plan name
1038	Partern name
1040	Material
1041	Height
1045	Length
1046	L_Surplus
1047	Width
1048	V_Surplus
1050	Saw  
7000	Start emluator
7001	In processing,the print setting is disable.
7002	NO. %3d group data  
7003	Width = %lf Length = %lf Height = %lf 
7004	The %3d th machining length %7.2f  
7005	Cutting side %7.2f  
7006	The %3d th maching number %d 
7007	Surplus material %7.2f  
7008	Code output of the %d block ：
7009	Machining data is error！
7010	Stop emluator
7011	No pattern data
7012	Emluator
7013	Start emluator
7014	Alarm：
7015	Alarm：None
7016	Working station：
7017	Normal
7018	Selected
7019	Unselected
7020	Start failure recovery
7021	Stop failure recovery
7022	Operating instructions
7023	Automatic layout 
7024	Running
7025	Running emluator
7026	Manual partern
7027	Input/output signal
7028	Commissioning
7029	Log
7030	Manual control
7031	Machine parameter setting
7032	clear failure
7033	Status
7034	Running status
7035	Current time
7036	Working hours
7037	Code：
7038	Name：
7039	Client：
7040	Customer：
7041	Material：
7042	Cut _S：
7043	Edge_M：
7044	Edge_S：
7045	5th program：
7046	6th program：
7047	Product name:
7048	Width edge
7049	Length edge
7050	Cut_L ：