1088	Manual operation
1078	Saw start 
1080	Main saw up
1081	Main saw down
1082	Saw forward
1119	Saw back
1314	Transom operation
1124	Front transom up/down
1125	Back transom up/down
1126	Sheild up/down
1313	Backboard operation
1133	Backboard Motor forward
1134	Backboard Motor back
1135	Front backboard down 
1136	Back backboard down 
1316	Maintance operation
1145	Fan run
1147	Lubrication
1148	Change the saw blade
1159	Clamp return RPS
1160	Clamp forward
1161	Clamp back
1162	Clamp reback working zero
1163	Clamp To set the location(50--3600)
1168	Clamp closed
1311	Clamp operation
1294	Position display
1297	Clamp Target position
1301	Saw Current position 
1302	Backboard Current position
1303	Saw operation
1306	Single cycle width (200-3300)
1307	Cutting speed set(10-50)
1308	Saw running speed 
1205	Saw return RPS
1036	Current working station ：Manual mode
1225	Alarm ：6 Fault of SUB-Blade upper bound
1309	Working mode 
1231	Manual mode
1232	Automatic mode
1022	Alarm Reset
1296	Current position of fixture
1304	Test the clamp position (0-10)： 
1326	Oreintation  cycle movement
7000	Alarm：
7001	Alarm：None
7002	Current working status ：
7003	Main saw stop
7004	Main saw start 
7005	Front backboard down 
7006	Front backboard up 
7007	Back backboard down
7008	Back backbboard up
7008	Saw start 
7010	Saw stop
7011	The machine is on automatic mode , stop and switch to manual mode ?
7012	System instruction
7013	Start failure recovery
7014	Stop failure recovery
7015	Operating instructions
7016	Automatic layout
7017	Running
7018	Running emulator
7019	Manual layout
7020	Input/Output signal
7021	Commissioning
7022	Log
7023	Manual control
7024	Machine parameter setting
7025	Clear alarm station
7026	Status
7027	running status
7028	Current time
7029	Working hours
