M03 N03 M0.3 Adjust choice bit 
M04 N04 M0.4 Last dec bit 
M10 N10 M1.0 Pause and then restart choise bit 
M11 N11 M1.1 Pause at Board too long bit 
M13 N13 M1.3 Choice of CE bit 
M14 N14 M1.4 Choice of Time of Decreasing longer bit 
M15 N15 M1.5 Choice of single platen bit 
M20 N20 M2.0 Drag Motor return RPS bit  
M21 N21 M2.1 Drag Motor go forward bit  
M22 N22 M2.2 Drag Motor go back bit  
M23 N23 M2.3 Work holder return RPS bit  
M24 N24 M2.4 Work holder go forward bit  
M25 N25 M2.5 Work holder go back bit  
M26 N26 M2.6 Work holder go back setting length bit  
M27 N27 M2.7 The collet closed bit  
M30 N30 M3.0 Motor of backup plate go forward bit  
M31 N31 M3.1 Motor of backup plate go back bit  
M32 N32 M3.2 Backup plate seat movment bit  
M33 N33 M3.3 Front backup plate go down bit  
M34 N34 M3.4 Back backup plate go down bit  
M35 N35 M3.5 Front platen go down bit  
M36 N36 M3.6 Back platen go down bit  
M37 N37 M3.7 Protective cover movement bit 
M40 N40 M4.0 Pump Lubrication oil bit  
M41 N41 M4.1 Change the saw blade bit  
M42 N42 M4.2 Auto running bit 
M43 N43 M4.3 Adjust test bit 
M44 N44 M4.4 First tool pause bit 
M45 N45 M4.5 Residual material in the front bit 
M46 N46 M4.6 Fence select bit 
M47 N47 M4.7 Work hloder to Projectting zero bit 
M51 N51 M5.1 Head auto down bit 
M52 N52 M5.2 Unusing bit 
M53 N53 M5.3 Hold_stop bit 
M54 N54 M5.4 Restart running bit 
M55 N55 M5.5 Work running bit 
M56 N56 M5.6 Fence select bit 
M57 N57 M5.7 Unusing bit 
M60 N60 M6.0 Manual mode bit 
M61 N61 M6.1 Automatic mode bit 
M62 N62 M6.2 Main saw running bit 
M63 N63 M6.3 Main saw running bit 
M64 N64 M6.4 Fan running bit 
M65 N65 M6.5 Main saw Cylinder up bit 
M66 N66 M6.6 Main saw Cylinder down bit 
M67 N67 M6.7 Unusing bit 
M113 N113 M11.3 Single cycle running bit 
M115 N115 M11.5 Auto cycle running bit 
M300 M30.0 M30.0 Download finished bit  
M05 N05 M0.5 Display mode bit 